Robot troubleshooting

--when program isn’t working as you expect it when following the logic, check wire connections. If a wire is loose the program won’t work right AND won’t give any error messages.